# Creo Parametric (Plug-in) Exporter

Section Name [ENF2PRO]

## UseOriginalUnitsystem

Specify whether to convert the unit system.
This is to set a loop-back when converting the unit system in Creo Parametric to Creo Parametric conversion.
“UseTemplateFile=1” will be prioritized to this parameter. (The unit system in the template file will be used.)

- Default Value: 0
- Values
  - 0: Don’t convert the unit system
  - 1: Convert the unit system

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties

## XConvertSystemProperty

Specify whether to convert system properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert system properties
  - 1: Convert system properties

## ImportAsMultiSolidBody

Specify whether to convert volumes as multiple bodies when converting to Creo 7.0 or later.

- Default Value: 1
- Values
  - 0: Convert as a single body
  - 1: Convert as multiple bodies

## ImportLevel

Specify the element to convert.

- Default Value: 1
- Values
  - 0: VOLUME, QUILT
  - 1: VOLUME, QUILT, DTM PLANE, DTM CURVE, DTM POINT

## MakeSolidFromImportFeat

Specify the method to covert solid model as solid or quilt

- Default Value: -1
- Values
  - -1: Convert solid model as solid(Convert topologically-closed shells without closed flag as quilt.)
  - 0: Convert solid model as quilt
  - 1: Convert solid model as solid(Convert all topologically-closed shells as solid.)

## ImportBlankedElement

Convert blanked element

- Default Value: 1
- Values
  - 0: Don’t convert blanked element
  - 1: Convert blanked element as blanked.
  - 2: Convert blanked element as unblanked.

## LayerNameOfDatumPointOfAxisAsHidden

Specify the hidden layer to add end datum points of datum axes to by its layer name.
This is to translate end datum points of datum axes which are produced during the translation process as hidden elements by moving them into hidden layers to maintain the visualization.
The specified layer will be changed to hidden if shown.
A new hidden layer will be created when there is no layer under the specified name.

- Default Value:

## ConvertPartwise

Specify whether to run the conversion with memory-saving mode.

- Default Value: 0
- Values
  - 0: Don’t enable memory saving mode
  - 1: Enable memory saving mode

## UseTemplateFile

Specify whether to convert using a template file.
Please ensure to specify the template file with either “TemplatePart” / “TemplateAsm”, or a config keyword “TEMPLATE_PART” / “TEMPLATE_ASSEMBLY”.
The config keyword will be prioritized when set in combination with “TemplatePart” / “TemplateAsm”.

- Default Value: 1
- Values
  - 0: Don’t use the template file
  - 1: Convert using the template file

## TemplatePart

Specify the template file for part models.

- Default Value:

## TemplateAsm

Specify the template file for assembly models.

- Default Value:

## RegenerateRelation

Specify whether to regenerate relations defined in the template file.

- Default Value: 0
- Values
  - 0: Don’t regenerate relations
  - 1: Regenerate relations

## ImportTol

Specify the import tolerance (Unit: mm)
Set a positive real number between 0.00001 and 0.1
This parameter will be prioritized when both this and “UseVolumeTol” are set.

- Default Value: 0.01

## UseVolumeTol

Specify the tolerance to import.

- Default Value: 0
- Values
  - 0: Import by 0.01mm.
  - 1: Import by volume tolerance.

## GenerateQAReport

Specify whether to generate a QA report on data translation.

- Default Value: 0
- Values
  - 0: Don’t generate QA report
  - 1: Generate QA report

## CalcMassProperty

Specify whether to convert the mass properties (volume, surface area, gravity and density), and output volume, surface area, and gravity to XML log.

- Default Value: 0
- Values
  - 0: Don’t output mass properties
  - 1: Output mass properties

## CalcElementNumber

Specify whether to output the number of elements to the XML log file.

- Default Value: 0
- Values
  - 0: Don’t output the number of elements
  - 1: Output the number of elements

## OverwriteSameNameParameter

Overwrite parameters with the same name. Available only when converting properties by XConvertUserProperty=1 or XConvertSystemProperty=1.

- Default Value: 0
- Values
  - 0: Rename parameters with the same name
  - 1: Overwrite parameters with the same name

## SkipEmptyValueParameter

Specify whether to skip parameter conversion when it is empty.
This is effective only when “XConvertUserProperty=1” or “XConvertSystemProperty=1”.

- Default Value: 0

- Values

  - 0: Don’t skip
    (Convert empty value parameters)
  - 1: Skip
    (Don’t convert empty value parameters)

## AddParameterDesignation

Add designation property to converted parameters. Available only when converting properties by XConvertUserProperty=1 or XConvertSystemProperty=1.

- Default Value: 0
- Values
  - 0: Do not add designation property
  - 1: Add designation property

## ProductMode

Specify whether to apply CADdoctor default setting

- Default Value: 0
- Values
  - 0: ASFALIS mode
  - 1: CADdoctor mode