# Creo View Exporter

Section Name [ENF2PV]

## ConvertTransparency

Specify whether to convert the transparency.

- Default Value: 1
- Values
  - 0: Don’t convert the transparency (Convert the transparency as 0%)
  - 1: Convert the transparency

## ConvertAnalyticSurfaceType

Specify the analytic surface types to convert as the analytic surface. Those that are not selected will be converted as general surfaces.
Multiple selection is available by specifying the sum of corresponding values.

- Default Value: 31
- Values
  - 1: Plane
  - 2: Sphere
  - 4: Cylinder
  - 8: Cone
  - 16: Torus
  - 32: Revolution
  - 64: Tabcyl

## ConvertAnalyticCurveType

Specify the analytic curve types to convert as the analytic curve. Those that are not selected will be converted as general curves.
Multiple selection is available by specifying the sum of corresponding values.

- Default Value: 7
- Values
  - 1: Line
  - 2: Circle
  - 4: Ellipse

## SaveMemory

Specify whether to run the conversion with memory-saving mode.

- Default Value: 0
- Values
  - 0: Don’t enable memory-saving mode
  - 1: Enable memory saving mode

## AssignFileNameToTopAssemblyName

Specify the name (assembly name in ENF or filename) to use for the top assembly name.

- Default Value: 0
- Values
  - 0: Use the assembly name in ENF
  - 1: Use the filename