# Mid Surfacer

Section Name [MIDSURFACE]

## MaxThickness

Specify the maximum wall thickness for pairing faces.
Specify by a positive real number.

- Default Value:

## FilletMaxRadius

Specify the maximum radius for fillet detection.
Specify by a positive real number.
This is set to the same value of “MaxThickness” by default.

- Default Value:

## BossMaxDiameter

Specify the maximum diameter for boss detection.
Specify by a positive real number.
This is set to five times of the value of “MaxThickness” by default.

- Default Value:

## IgnoreFillet

Specify whether to ignore fillets in midsurface generation.

- Default Value: 1

- Values

  - 0: Don’t ignore
    (Keep fillets)

  - 1: Ignore fillets, and create sharp corners

## IgnoreBoss

Specify whether to ignore bosses in midsurface generation.

- Default Value: 1

- Values

  - 0: Don’t ignore
    (Keep bosses)

  - 1: Ignore bosses

## CleanupShortCurveTolerance

Specify the short curve tolerance for fixing short curves (by merging or extending).
Specify by a positive real number.

- Default Value: 0.1

## ExportByParts

Specify whether to export the result files divided by part.

- Default Value: 0

- Values

  - 0: Don’t divide
    (Export all parts in a single file)

  - 1: Export in file(s) divided by part

## ExportByThickness

Specify whether to export the result files divided by the wall thickness.

- Default Value: 0

- Values

  - 0: Don’t divide
    (Export in a single file regardless of the wall thickness)

  - 1: Export in file(s) divided by wall thickness

## PrecisionToClassifyThickness

Specify the tolerance to regard as the same wall thickness.
Specify by a positive real number.
This is effective only when “ExportByThickness=1”.

- Default Value: 0.1