# PLM XML Importer

Section Name [PLMXML2ENF]

## ConvertJTPart

Specify whether to convert externally referenced files in JT format.

- Default Value: 0
- Values
  - 0: Don’t convert externally referenced files in JT format (Ignore them)
  - 1: Convert externally referenced files in JT format

## ConvertNXPart

Specify whether to convert the external reference part files in NX format.

- Default Value: 0
- Values
  - 0: Don’t convert the external reference parts in NX format
  - 1: Convert the external reference part files in NX format

## HealExternalFile

Specify whether to run automatic geometry healing on externally referenced files.
It is recommended to turn off this parameter when the output ENF file is to be used for CAD validation.

- Default Value: 1
- Values
  - 0: Don’t heal externally referenced files (Recommended when validating PLM XML file vs. CAD file)
  - 1: Heal externally referenced files (Recommended when translating PLM XML to CAD)

## SkipEmptyAsmExternalFile

Specify whether to skip translating the assembly external file when it is empty

- Default Value: 0

- Values

  - 0: Don’t skip
    (Translate the assembly external file even when it is empty)

  - 1: Skip translating the assembly external file when it is empty

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties. In case of a key name conflict, convert using the value in PLM XML.
  - 2: Convert user properties. In case of a key name conflict, convert using the value in external reference part files.

## FlattenPartNode

Specify whether to flatten the tree structure when converting Part Node which has a single Compoundrep Node only.

- Default Value: 1

- Values

  - 0: Don’t flatten
    (Maintain the tree structure and convert Part Node as assemblies and Compondrep Node as parts)
  - 1: Flatten the tree structure
    (Merge Compoundrep Node to its parent Part Node and convert as a single part)