# CATIA V4 Importer

Section Name [CATIA2ENF]

## ElementType

Specify whether to convert per element type.
Specify by an 8-digit integer (abcdefgh) which each digit corresponds to the following element type respectively;
—–
a: Solid
b: Volume
c: Skin
d: Face
e: Surface
f: Curve
g: Point
h: *Reserved - Always set to zero
—–
The value for “a” is either of the followings, and the value for “b” to “g” is either “0: Don’t convert” or “1: Convert”.
0: Don’t convert
1: Convert SOLE
2: Convert SOLM
3: Convert SOLE and SOLM

- Default Value: 11111110

## AxisBody

Specify whether to delete bodies which have the axis only.

- Default Value: 0
- Values
  - 0: Don’t delete (Convert bodies which have axis only)
  - 1: Delete bodies which have axis only (Don’t convert)

## AxisSystem

Specify the coordinate system to use in conversion.

- Default Value: 1
- Values
  - 0: Absolute coordinate system
  - 1: Current coordinate system

## SuppressionType

This is used as query filter by display attributes.

- Default Value: 0
- Values
  - 0: Current Layer and SHOW
  - 1: Current Layer and SHOW/NOSHOW
  - 10: All Layer and SHOW
  - 11: All layer and SHOW/NOSHOW

## SimpleAssembly

Specify whether to simplify the assembly structure in conversion.
The assembly will not be created when there is no Ditto in DetailWorkSpace.

- Default Value: 0
- Values
  - 0: Don’t simplify the assembly structure
  - 1: Simplify the assembly structure

## StructureMode

Specify whether to convert the assembly structure only without part information.

- Default Value: 0
- Values
  - 0: Convert assembly structure + part information
  - 1: Convert assembly structure only

## ProductMode

Specify whether to apply CADdoctor default setting

- Default Value: 0
- Values
  - 0: ASFALIS mode
  - 1: CADdoctor mode

## XVLOption

Specify whether to use option for XVL (conversion of window, empty work space etc.).

- Default Value: 0
- Values
  - 0: Don’t use option for XVL
  - 1: Use option for XVL