# JT Exporter

Section Name [ENF2JT]

## FileVersion

Specify the JT version for data export.
Please note that the value for this parameter will be automatically replaced with “FileVersion=94” when parameters for PMI conversion are set, but JT version 9.3 or older is specified.

- Default Value: 95
- Values
  - 100: Export in JT version 10.0
  - 101: Export in JT version 10.1
  - 102: Export in JT version 10.2
  - 103: Export in JT version 10.3
  - 104: Export in JT version 10.4
  - 105: Export in JT version 10.5
  - 106: Export in JT version 10.6
  - 107: Export in JT version 10.7
  - 90: Export in JT version 9.0
  - 91: Export in JT version 9.1
  - 92: Export in JT version 9.2
  - 93: Export in JT version 9.3
  - 94: Export in JT version 9.4
  - 95: Export in JT version 9.5

## FileFormat

Specify the file format of exported JT file.

- Default Value: 2
- Values
  - 0: Export in MONOLITHIC (Export all in a single file)
  - 1: Export in FULL_SHATTER (Export in separate files per assembly / part)
  - 2: Export in PER_PART (Export in separate files per assembly / part, and place them in a sub folder except the top file)

## JtConfigPath

Specify the JT Configuration File.
The built-in config file in the Component installation folder will be used when this is not set.

- Default Value:

## Unit

Specify a unit.

- Default Value: 2
- Values
  - 2: Millimeter
  - 5: Meter
  - 7: Inch

## XConvertPMI

Specify whether to convert PMI.

- Default Value: 0
- Values
  - 0: Don’t convert PMI
  - 1: Convert PMI
  - 2: Convert as Graphic PMI

## XConvertView

Specify whether to convert the View.

- Default Value: 0
- Values
  - 0: Don’t convert View
  - 1: Convert View

## ConvertInvisiblePMI

Specify whether to convert hidden PMI.
This will be prioritized for hidden PMI conversion when set in combination with “ConvertInvisible”.
This is effective only when “XConvertPMI=1 or 2”.

- Default Value: 1
- Values
  - 0: Don’t convert hidden PMI
  - 1: Convert all PMI
  - 2: Don’t covert PMI which are hidden in all views

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties

## XConvertSystemProperty

Specify whether to convert system properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert system properties
  - 1: Convert system properties

## ConvertGeometryType

Specify the type of the geometry format to translate
Multiple selections is available by specifying sum of corresponding numbers.

- Default Value: 3
- Values
  - 1: Translate ENF B-rep to JT B-rep only
  - 2: Translate ENF B-rep to JT tessellate polygon only
  - 4: Translate ENF polygon to JT polygon
  - 8: If ENF has both B-rep and polygon for the same component, translate ENF B-rep to JT-tessellate polygon (ignore ENF polygon)

## ConvertIsoCurve

Specify whether to convert isolated wireframe curves.

- Default Value: 1
- Values
  - 0: Don’t convert isolated curves
  - 1: Convert isolated curves

## ConvertIsoPoint

Specify whether to convert isolated points.

- Default Value: 2
- Values
  - 0: Don’t convert isolated points.
  - 1: Convert isolated points.
  - 2: Convert isolated points as reference points.

## ConvertRefPlane

Convert Reference Plane.
Multiple selection is available by specifying the sum of corresponding values.

- Default Value: 1
- Values
  - 1: Convert reference plane
  - 2: Convert default plane

## ConvertRefAxis

Convert Reference Axis

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertRefPoint

Specify whether to convert reference points.

- Default Value: 1
- Values
  - 0: Don’t convert reference points.
  - 1: Convert reference points.

## ConvertCSys

Convert Coordinate Systems

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertEmptyBodyNode

Control the convertion of empty body node.
Available only when ConvertBodyNode=1 or 2 is specified.

- Default Value: 1
- Values
  - 0: Convert only body node which has geometry.
  - 1: Convert all body node.

## ConvertBodyNode

[CATIA V5 to JT Conversion]
Specify whether to create body nodes, and the level for the creation (each body, geometrical set, UDF and geometry feature).
[JT to JT Conversion]
Specify whether to maintain the body node structure. The behavior is the same when set to 1 or 2.
[Other CAD Formats to JT Conversion]
Specify whether to create body nodes for each volume and isolated element.
When converting from other formats, body nodes will be created for each volume and isolated element. The behavior is the same when set to 1 or 2.

- Default Value: 1

- Values

  - 0: Don’t create body nodes

  - 1: Create body nodes
    [From CATIA V5]: For each body, geometrical set, and UDF only
  - 2: Create body nodes
    [From CATIA V5]: For each body, geometrical set, UDF and geometry feature
  - 3: Create body nodes, but limit the tree structure depth to no more than two
    [From CATIA V5]: For each body, geometrical set, and UDF only

## ConvertInvisible

Specify whether to convert hidden elements.
You can also tune up with the following parameter, which will be prioritized to this when set in combination;
- ConvertInvisibleInstance: Hidden instances

- Default Value: 0
- Values
  - 0: Don’t convert hidden elements
  - 1: Convert hidden elements

## ConvertInvisibleInstance

Specify whether to convert hidden instances.
This will be prioritized for hidden instance conversion when set in combination with parameter “ConvertInvisible”.

- Default Value: -1

- Values

  - -1: Apply the settings specified with parameter “ConvertInvisible”
    (Effective only when “ConvertInvisible” is set.)

  - 0: Don’t convert hidden instances

  - 1: Convert hidden instances

## ConvertLayerFilter

Specify whether to convert layer filters and layer numbers.
The layer number is supported on the body node, wire (isolated curve), PMI, reference plane, reference axis, reference point and coordinate system.

- Default Value: 1
- Values
  - 0: Don’t convert layer filters and layer numbers
  - 1: Convert layer filters and layer numbers

## RemoveSeamCurve

Specify surface types to remove seam curves.
Multiple selection is available by specifying the sum of corresponding values.
Settings for Geometry Healing will be applied when this is not set.

- Default Value: -1
- Values
  - -1: Remove seam curves based on settings for Geometry Healing
  - 0: Don’t remove seam curves
  - 1: Remove seam curves on spherical surfaces
  - 2: Remove seam curves on cylindrical surfaces
  - 4: Remove seam curves on conic surfaces
  - 8: Remove seam curves on torus surfaces

## SaveMemory

Specify whether to run the conversion with memory-saving mode.

- Default Value: 0
- Values
  - 0: Don’t enable memory-saving mode
  - 1: Enable memory saving mode

## EltessChordalTol

Specify chordal tolerance for Elysium tessellator (mm)
Positive real number value

- Default Value: 1.0

## EltessAngularTol

Specify angular tolerance for Elysium tessellator (degree)
Positive real number value

- Default Value: 15.0

## UseEltess

Specify whether to convert using the Elysium tessellator.

- Default Value: 0
- Values
  - 0: Convert using JT tesselator, and retry with Elysium tesselator when failed
  - 1: Convert using Elysium tesselator

## ReplaceNXProhibitChar

Specify whether to replace characters prohibited in NX by underscores (“_”).

- Default Value: 2
- Values
  - 0: Don’t replace
  - 1: Replace characters prohibited in NX9 or earlier
  - 2: Replace characters prohibited in NX10 or later

## GenerateQAReport

Specify whether to generate QA (Quality Assurance) reports on data translation.

- Default Value: 0
- Values
  - 0: Don’t generate a QA report.
  - 1: Generate a QA report.

## XConvertNote

Specify whether to convert Note. (PMI)

- Default Value: -1
- Values
  - -1: Follow the translation settings set with “XConvertPMI”
  - 0: Don’t convert Note
  - 1: Convert Note
  - 2: Convert as Graphic PMI

## XConvertDimension

Specify whether to convert Dimension. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Dimension
  - 1: Convert Dimension
  - 2: Convert as Graphic PMI

## XConvertGDT

Specify whether to convert GDT, Datum and DatumTarget. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert GDT
  - 1: Convert GDT
  - 2: Convert as Graphic PMI

## XConvertSurfFinish

Specify whether to convert SurfaceFinish. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert SurfaceFinish
  - 1: Convert SurfaceFinish
  - 2: Convert as Graphic PMI

## XConvertLineWeld

Specify whether to convert LineWeld. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Line Weld
  - 1: Convert Line Weld
  - 2: Convert as Graphic PMI

## XConvertSpotWeld

Specify whether to convert SpotWeld. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Spot Weld
  - 1: Convert Spot Weld
  - 2: Convert as Graphic PMI

## XConvertLocator

Specify whether to convert Locator. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Locator
  - 1: Convert Locator
  - 2: Convert as Graphic PMI

## XConvertSymbol

Specify whether to convert PMI without semantic definition to Custom Symbol PMI.

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert
  - 1: Convert to Custom Symbol

## ConvertPMIAutoFlip

Specify whether to convert PMI with auto-flip of PMI text enabled.
This is effective only when PMI translation is enabled with “XConvert***” parameter(s).

- Default Value: 1
- Values
  - 0: Convert PMI with auto-flip disabled
  - 1: Convert PMI with auto-flip enabled

## ShowOtherPartsInModelView

Show parts in the model view’s scope that are not specifically mentioned in the model view.

- Default Value: 1
- Values
  - 0: Hide other parts
  - 1: Show other parts

## FlattenView

Specify whether to flatten Model Views and skip creating View Sets.

- Default Value: 0

- Values

  - 0: Don’t flatten Model View
    (View Sets will be created)

  - 1: Flatten Model View

## TranslatorInformation

Specify whether to convert translator information.

- Default Value: 1
- Values
  - 0: Don’t convert translator information.
  - 1: Convert translator information.