# JT Importer

Section Name [JT2ENF]

## XConvertPMI

Specify whether to convert PMI.

- Default Value: 0
- Values
  - 0: Don’t convert PMI
  - 1: Convert PMI

## XConvertView

Specify whether to convert View.

- Default Value: 0
- Values
  - 0: Don’t convert View
  - 1: Convert View

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties
  - 2: Convert public user properties only
  - 3: Convert user public properties except those automatically generated in JT

## ConvertGeometryType

Specify the type of the geometry format to convert.
Multiple selection is available by specifying the sum of corresponding values.
Use “Recover Flag” to convert the other type when the specified type does not exist in the input file.
e.g., “ConvertGeometryType=9 (=1+8)” means to usually convert polygon, but convert B-rep instead when polygon does not exist.

- Default Value: 3

- Values

  - 1: Convert polygon only

  - 2: Convert B-rep (XT B-rep and native B-rep) only

  - 8: Set Recover Flag
    (Convert the other type when specified type does not exist in the input file)

## ConvertGeneralBody

Convert general body

- Default Value: 0
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertRefPlane

Convert Reference Plane

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertRefAxis

Convert Reference Axis

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertRefPoint

Specify whether to convert reference points.

- Default Value: 1
- Values
  - 0: Don’t convert reference points.
  - 1: Convert reference points.

## ConvertCSys

Convert Coordinate Systems

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert

## ConvertPolygonPointSetAsVertex

Specify whether to convert polygon points to vertices.
Polygon points will be converted as polygon points regardless whether converting to vertices when polygon is in scope of conversion with “ConvertGeometryType”.

- Default Value: -1
- Values
  - -1: Convert to vertices when B-rep is in scope of conversion with “ConvertGeometryType” and B-rep exists in the JT file
  - 0: Don’t convert to vertices
  - 1: Convert to vertices

## FlattenBodyNode

Specify how the body node should be converted.

- Default Value: 1
- Values
  - 0: Convert the structure of body node to the assembly structure tree, and the leaf body nodes to parts
  - 1: Merge the body node to its parent part node, and convert them as a single part. Convert body nodes as Feature Groups.
  - 2: Merge the body node to its parent part node and convert them as a single part. Do not convert body nodes as Feature Groups.

## ForceBodyNode

Specify nodes that are not Body Node in JT, but to treat as Body Node. They will be converted to elements under part in ENF.
Please ensure to specify nodes by their names with “ForceBodyNodeFile” when this is set to “1”.

- Default Value: 0
- Values
  - 0: None (Only Body Nodes in source JT file will be converted as Body Nodes.)
  - 1: Nodes specified by name with “ForceBodyNodeFile”
  - 2: All nodes except for the top node

## ForceBodyNodeFile

Specify the node name list (file that lists node names to treat as Body Node by their names).
Recommended settings (“ForceBodyNode.txt” in the installation folder) will be used when this is not set.
This is effective only when “ForceBodyNode=1”.

- Default Value:

## ConvertLayerFilter

Specify whether to convert layer filters and layer numbers.
The layer number is supported on the body node, wire (isolated curve), PMI, reference plane, reference axis, reference point and coordinate system.

- Default Value: 1
- Values
  - 0: Don’t convert layer filters and layer numbers
  - 1: Convert layer filters and layer numbers

## LOD

Select LOD in JT file to be converted.
1-origin Integer. 1 means the minutest polygon. Getting rougher as a value increases.

- Default Value: 1

## XConvertNote

Specify whether to convert Note. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Note
  - 1: Convert Note

## XConvertDimension

Specify whether to convert Dimension. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Dimension
  - 1: Convert Dimension

## XConvertGDT

Specify whether to convert GDT, Datum and DatumTarget. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert GDT
  - 1: Convert GDT

## XConvertSurfFinish

Specify whether to convert SurfaceFinish. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert SurfaceFinish
  - 1: Convert SurfaceFinish

## XConvertLineWeld

Specify whether to convert LineWeld. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Line Weld
  - 1: Convert Line Weld

## XConvertSpotWeld

Specify whether to convert SpotWeld. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Spot Weld
  - 1: Convert Spot Weld

## XConvertLocator

Specify whether to convert Locator. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Locator
  - 1: Convert Locator

## XConvertSymbol

Specify whether to convert Custom Symbol. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Custom Symbol
  - 1: Convert Custom Symbol

## XConvertGraphicDataPMI

Specify whether to convert graphic PMIs such as center line and region as graphic PMIs.

- Default Value: -1
- Values
  - -1: Follow the convert settings set with “XConvertPMI”
  - 0: Don’t convert
  - 1: Convert as graphic PMI