# Creo Parametric (Plug-in) Importer

Section Name [PRO2ENF]

## UseOriginalUnitsystem

Specify whether to convert the unit system.
This is to set a loop-back when converting the unit system in Creo Parametric to Creo Parametric conversion.

- Default Value: 0
- Values
  - 0: Don’t convert the unit system
  - 1: Convert the unit system

## AbsoluteCS

Select reference coordinate system
none:
Convert with default coordinate system.
Coordinate System name:
Convert with specified coordinate system.

- Default Value:

## XConvertPMI

Specify whether to convert PMI.

- Default Value: 0
- Values
  - 0: Don’t convert PMI
  - 1: Convert PMI

## XConvert3DAnnotationAsPolyline

Specify whether to also convert as polyline PMI when converting PMI as semantic PMI.

- Default Value: 1
- Values
  - 0: Don’t convert as polyline PMI (Convert as semantic PMI only)
  - 1: Convert as polyline PMI as well

## XConvertView

Specify whether to convert the View.

- Default Value: 0
- Values
  - 0: Don’t convert View
  - 1: Convert View

## XConvertFlatToScreenAF

Specify how to convert flat-to-screen annotations.
This is effective only when annotation translation is enabled with one or more of the followings;
- “XConvertNote=1”
- “XConvertGDT=1”
- “XConvertSurfFinish=1”

- Default Value: 1
- Values
  - 0: Don’t convert flat-to-screen annotations
  - 1: Convert flat-to-screen annotations seen from the default orientation
  - 2: Convert flat-to-screen annotations seen from the standard orientation

## ConvertPmiOnlyInCombstate

Specify whether to limit the target for PMI conversion to those that are included in Combined State only.
This is effective only when “XConvertPMI=1”.

- Default Value: 0
- Values
  - 0: Don’t limit (Convert all PMI)
  - 1: Limit to PMI included in Combined State only

## ConvertCombstate

Specify whether to convert combined state.

- Default Value: 0
- Values
  - 0: Don’t convert combined state
  - 1: Convert combined state that belong to top component only
  - 2: Convert all combined states

## ConvertCombstateOnlyPublishing

Specify whether to limit the target for Combined State conversion to published ones only. (Combined States which are not published will not be converted.)
This is effective only when “ConvertCombstate=1 or 2”.

- Default Value: 0
- Values
  - 0: Don’t limit (Convert all Combined States regardless of “Publish” status)
  - 1: Limit to published Combined States only

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties

## XConvertMaterial

Specify whether to convert material properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert material properties
  - 1: Convert material properties

## ConvertGeometryType

Specify the geometry format to convert (convert Solid and Quilt of input Creo Parametric file as B-rep, or obtain them in polygon format and convert to polygon in ENF).
Please note that DatumPoint, DatumAxis, DatumCurve and DatumPlane will not be converted when this is set to “1”.

- Default Value: 0
- Values
  - 0: Convert Solid and Quilt as B-rep
  - 1: Convert Solid and Quilt obtained in polygon format to polygon (B-rep will not be converted)

## ConvertSolid

Convert Solid

- Default Value: 1
- Values
  - 0: Don’t convert Solid.
  - 1: Convert Solid.

## ConvertHarness

Specify whether to convert harnesses.

- Default Value: 1
- Values
  - 0: Don’t convert harness.
  - 1: Convert harness.

## ConvertQuilt

Convert Quilt

- Default Value: 1
- Values
  - 0: Don’t convert Quilt.
  - 1: Convert Quilt.

## ConvertDtmCv

Specify whether to convert DatumCurve.

- Default Value: 1
- Values
  - 0: Don’t convert DatumCuve
  - 1: Convert DatumCurve

## ConvertDtmPl

Specify whether to convert DatumPlane.

- Default Value: 0
- Values
  - 0: Don’t convert DatumPlane
  - 1: Convert DatumPlane

## ConvertDtmAx

Specify whether to convert axis.

- Default Value: 0
- Values
  - 0: Don’t convert axis
  - 1: Convert axis

## ConvertDtmPt

Specify whether to convert DatumPoint.

- Default Value: 1
- Values
  - 0: Don’t convert DatumPoint
  - 1: Convert DatumPoint

## ConvertDtmCs

Specify whether to convert Csys.

- Default Value: 0
- Values
  - 0: Don’t convert Csys
  - 1: Convert Csys

## ConvertSkeletonModel

Specify whether to convert skeleton models.

- Default Value: 1
- Values
  - 0: Don’t convert
  - 1: Convert skeleton models

## ConvAsmBdy

Specify whether to create a derived body to convert elements that belong to an assembly (*.asm) to it.

- Default Value: 1
- Values
  - 0: Don’t convert assembly elements
  - 1: Create a derived body and convert assembly elements to it

## ConvertThreadQuilt

Specify whether and how to convert hidden (blanked) Quilt created by Cosmetic Thread or Hole feature.

- Default Value: 0
- Values
  - 0: Don’t convert
  - 1: Convert as hidden Quilt
  - 2: Convert as shown Quilt

## ExportBlankedElement

Specify whether to convert hidden (blanked) elements.
Please note that “ExportBlankedComponent” / “ExportBlankedQuilt” / “ExportBlankedSolid” will be prioritized when they are set.

- Default Value: 1
- Values
  - 0: Don’t convert hidden elements
  - 1: Convert hidden elements as hidden elements
  - 2: Convert hidden elements as shown elements

## ExportBlankedComponent

Specify whether to convert hidden (blanked) Component.
This will be prioritized to “ExportBlankedElement” when both set.

- Default Value: -1

- Values

  - -1: Convert based on the settings specified with “ExportBlankedElement”
    (Effective only when “ExportBlankedElement” is set.)

  - 0: Don’t convert hidden Component

  - 1: Convert hidden Component as hidden Component

  - 2: Convert hidden Component as shown Component

## ExportBlankedSolid

Specify whether to convert hidden (blanked) solid volumes.
This will be prioritized to “ExportBlankedElement” when both set.

- Default Value: -1
- Values
  - -1: Convert based on the settings specified with “ExportBlankedElement”
  - 0: Don’t convert hidden solid volumes
  - 1: Convert hidden solid volumes as hidden solid volumes
  - 2: Convert hidden solid volumes as shown solid elements

## ExportBlankedQuilt

Specify whether to convert hidden (blanked) Quilt.
This will be prioritized to “ExportBlankedElement” when both set.

- Default Value: -1
- Values
  - -1: Convert based on the settings specified with “ExportBlankedElement”
  - 0: Don’t convert hidden Quilt
  - 1: Convert hidden Quilt as hidden Quilt
  - 2: Convert hidden Quilt as shown Quilt

## ConvFamInst

Specify whether to convert specified family instances.
Specify
- Empty string: Convert generic instance (Don’t convert family instances)
- Family instance name: Convert specified family instance

- Default Value:

## SimplifiedRep

Specify whether to convert with simplified representation specified by its name.
Please note that this supports user defined simplified representation names only.
It will be converted with master representation when this is not set.

- Default Value:

## SimplifiedRepRecoverMode

Specify whether to convert by Master Rep when the input file cannot be read by the simplified representation specified by “SimplifiedRep”.

- Default Value: 0
- Values
  - 0: Don’t convert by Master Rep, and return error
  - 1: Convert by Master Rep

## ConvertPartwise

Specify whether to run the conversion with memory-saving mode.

- Default Value: 0
- Values
  - 0: Don’t enable memory saving mode
  - 1: Enable memory saving mode

## StructureMode

Specify whether to convert the assembly structure only without part information.

- Default Value: 0
- Values
  - 0: Convert assembly structure + part information
  - 1: Convert assembly structure only

## CalcMassProperty

Specify whether to convert the mass properties (volume, surface area, gravity and density), and output volume, surface area, and gravity to XML log.

- Default Value: 0
- Values
  - 0: Don’t output mass properties
  - 1: Output mass properties

## CalcElementNumber

Specify whether to output the number of elements to the XML log file.

- Default Value: 0
- Values
  - 0: Don’t output the number of elements
  - 1: Output the number of elements

## XConvertNote

Specify whether to convert Note. (PMI)

- Default Value: -1
- Values
  - -1: Follow the translation settings set with “XConvertPMI”
  - 0: Don’t convert Note
  - 1: Convert Note

## XConvertDimension

Specify whether to convert Dimension. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert Dimension
  - 1: Convert Dimension

## XConvertGDT

Specify whether to convert GDT, Datum and DatumTarget. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert GDT
  - 1: Convert GDT

## XConvertSurfFinish

Specify whether to convert SurfaceFinish. (PMI)

- Default Value: -1
- Values
  - -1: Follow the conversion settings set with “XConvertPMI”
  - 0: Don’t convert SurfaceFinish
  - 1: Convert SurfaceFinish

## ProductMode

Specify whether to apply CADdoctor default setting

- Default Value: 0
- Values
  - 0: ASFALIS mode
  - 1: CADdoctor mode