# NX I-deas Importer

Section Name [IDEAS2ENF]

## XConvertNote

Specify whether to convert Note. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert Note
  - 1: Convert Note

## XConvertDimension

Specify whether to convert Dimension. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert Dimension
  - 1: Convert Dimension

## XConvertGDT

Specify whether to convert GDT, Datum, DatumTarget. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert GDT
  - 1: Convert GDT

## XConvertSurfFinish

Specify whether to convert SurfaceFinish. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert SurfaceFinish
  - 1: Convert SurfaceFinish

## XConvertLineWeld

Specify whether to convert LineWeld. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert LineWeld
  - 1: Convert LineWeld

## XConvertSpotWeld

Specify whether to convert SpotWeld. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert SpotWeld
  - 1: Convert SpotWeld

## XConvertLocator

Specify whether to convert Locator. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert Locator
  - 1: Convert Locator

## XConvertHatching

Specify whether to convert Hatching. (PMI)

- Default Value: 0
- Values
  - 0: Don’t convert Hatching
  - 1: Convert Hatching

## XConvertSection

Specify whether to convert sections.

- Default Value: 0
- Values
  - 0: Don’t convert sections
  - 1: Convert sections

## XConvert3DAnnotationAsPolyline

Specify whether to also convert as polyline PMI when converting PMI as semantic PMI.

- Default Value: 1
- Values
  - 0: Don’t convert as polyline PMI (Convert as semantic PMI only)
  - 1: Convert as polyline PMI as well

## XConvertView

Specify whether to convert the View.

- Default Value: 0
- Values
  - 0: Don’t convert View
  - 1: Convert View

## XConvertUserProperty

Specify whether to convert user properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert user properties
  - 1: Convert user properties

## XConvertSystemProperty

Specify whether to convert system properties. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert system properties
  - 1: Convert system properties

## XConvertMaterial

Specify whether to convert Material. (Attribute)

- Default Value: 0
- Values
  - 0: Don’t convert Material
  - 1: Convert Material

## GetAllPart

Specify whether to convert all parts in BIN folder.
Please note that all data in BIN folder will be converted regardless of the value of this parameter when the data in BIN folder are parts only (no assembly).

- Default Value: 0

- Values

  - 0: Don’t convert parts in BIN folder
    (Parts in BIN folder will be converted anyway when there are parts only, and no assemblies.)

  - 1: Convert all parts in BIN folder

## SupportWFPoint

Specify whether to convert isolated points.
This is effective only when “UseOiMode=0” (default option).
Isolated points will always be converted when “UseOiMode=1”.

- Default Value: 0
- Values
  - 0: Don’t convert isolated points
  - 1: Convert isolated points

## WriteHideInstance

Specify whether to translate hidden instances

- Default Value: 0
- Values
  - 0: Don’t translate hidden instances
  - 1: Translate hidden instances as shown instances
  - 2: Translate hidden instances as hidden instances

## WriteSuppressInstance

Specify whether to translate Suppress Instances

- Default Value: 0
- Values
  - 0: Don’t translate Suppress Instances
  - 1: Translate Suppress Instances as shown instances
  - 2: Translate Suppress Instances as hidden instances

## WriteAbstractInstance

Specify whether to translate the abstract instances.

- Default Value: 0
- Values
  - 0: Don’t translate the abstract instances
  - 1: Translate the abstract instances as shown instances
  - 2: Translate the abstract instances as hidden instances

## WritePruneInstance

Specify whether to translate Prune Instances

- Default Value: 0
- Values
  - 0: Don’t translate Prune Instances
  - 1: Translate Prune Instances as shown instances
  - 2: Translate Prune Instances as hidden instances

## ConvertPartwise

Specify whether to run the conversion with memory-saving mode.

- Default Value: 0
- Values
  - 0: Don’t enable memory saving mode
  - 1: Enable memory saving mode

## StructureMode

Specify whether to convert the assembly structure only without part information.

- Default Value: 0
- Values
  - 0: Convert assembly structure + part information
  - 1: Convert assembly structure only

## UseOiMode

Specify whether to convert using OI function to convert maintaining the face transparency. (The face transparency will be lost when converting with IDI function.)
Please note that the arrow of PMI and some elements will be lost when converting with OI function.

- Default Value: 0
- Values
  - 0: Convert using IDI function
  - 1: Convert using OI function

## CalcMassProperty

Specify whether to output the mass properties (volume, surface area, and center of gravity) to the XML log file.

- Default Value: 0
- Values
  - 0: Don’t output mass properties
  - 1: Output mass properties

## CalcElementNumber

Specify whether to output the number of elements to the XML log file.

- Default Value: 0
- Values
  - 0: Don’t output the number of elements
  - 1: Output the number of elements

## SupportXVL

Specify whether to translate vector annotations (3D Polylines), cameras (Model Views) and material names
(This is the setting for the translation to XVL.)

- Default Value: 0
- Values
  - 0: Don’t translate vector annotations (3D Polylines), cameras (Model Views) and material names
  - 1: Translate vector annotations (3D Polylines), cameras (Model Views) and material names