# ACIS Exporter

Section Name [ENF2ACIS]

## AcisFileVer

Specify the version of ACIS file to export.

- Default Value: 32
- Values
  - 10: Export in version 10
  - 11: Export in version 11
  - 12: Export in version 12
  - 13: Export in version 13
  - 14: Export in version 14
  - 15: Export in version 15
  - 16: Export in version 16
  - 17: Export in version 17
  - 18: Export in version 18
  - 19: Export in version 19
  - 20: Export in version 20
  - 21: Export in version 21
  - 22: Export in version 22
  - 23: Export in version 23
  - 24: Export in version 24
  - 25: Export in version 25
  - 26: Export in version 26
  - 27: Export in version 27
  - 28: Export in version 28
  - 29: Export in version 29
  - 30: Export in version 30
  - 31: Export in version 31
  - 32: Export in version 32
  - 6: Export in version 6
  - 7: Export in version 7
  - 8: Export in version 8
  - 9: Export in version 9

## PointCoincidentTolerance

Specify point coincidence
Positive true number (However, it uses default value if it is less than 1e-6)

- Default Value: 0.000001

## TolerantModeling

Specify whether to enable the tolerant modeling in conversion.

- Default Value: 0
- Values
  - 0: Don’t enable tolerant modeling
  - 1: Enable tolerant modeling

## OutputEntity

Specify output entity

- Default Value: ALL
- Values
  - ALL: SOLID+WIRE
  - SOLID: Output Lump Entity
  - WIRE: Output Wire Entity

## SkipSeparate

Specify whether to export to ACIS using the same part and volume structure as ENF, instead of creating a part per Lump.

- Default Value: 0
- Values
  - 0: Create a part for each Lump
  - 1: Use the same part and volume structure as ENF (Don’t create a part for each Lump)

## ProductMode

Specify whether to apply CADdoctor default setting

- Default Value: 0
- Values
  - 0: ASFALIS mode
  - 1: CADdoctor mode